WeOS
5.29.0

# Jumbo Frame Switching

## Introduction

On certain platforms it is possible to enable switching (but only switching) of Jumbo Frames. Enabling this option sets the MTU discard policy for any ports associated with a VLAN to 9000 bytes.

    example:/#> configure
    example:/config/#> system
    example:/config/system/#> jumbo-frame-switching

The example above enables jumbo frame switching. It can be disable again by using `no jumbo-frame-switching` under `config/system`

`[no] jumbo-frame-switching`
  Enables switching of jumbo frames (up to 9000 bytes) on any ports associated with a VLAN.
no
  Disables jumbo frame switching

« Previous Next »