WeOS
5.29.0

# Switch management interfaces

## Introduction

The switch main configuration is stored in JSON format, however to manage the switch the following options are supported:

- Command line interface (CLI): The CLI can be accessed via Console, SSH and Telnet.
- Web interface: Web interface can be accessed via HTTP/HTTPS.
- SNMP (v1/v2c/v3): Currently limited to read-only operations and trap support; no general SNMP write support. See MIB conformance information in release zip for details.

## Configuration

Management services can be configured in the management configuration context.

    example:/#> configure
    example:/config/#> management
    example:/config/management/#>

From the management configuration context it is possible to enter specific sub-contexts to manage settings of individual services:

- `web`: Manage settings for the Web interface.
- `cli`: Manage general settings for the CLI. These settings apply to CLI, irrespective if accessed via Console, SSH or Telnet.
- `ssh`: Manage settings for the SSH service.
- `telnet`: Manage settings for the Telnet service.
- `snmp`: Manage SNMP settings.

« Previous Next »