WeOS
5.20.1

# AAA - Restricted interface

## About

If the user does not have administrator privileges the number of available commands are restricted.

## Example

Below is presented a list of commands available to a built-in user having a guest role.

    hostname:/#> whoami
    gertrude (guest)
    hostname:/#> help
    show alarm [log]    Alarm status, or show alarm log
    show arp            Show CPU ARP cache
    clear               Clear screen.
    show dhcp-clients   Show active DHCP clients. ...
    show sensor         Display environment status: temperature, power, digital in and SFP ...
    show fdb            Forwarding database (ATU/MAC)
    ip <igmp|ospf|..>   System IP mode commands
    show iface [..]     Interface overview
    show lldp           LLDP/CDP neighbours
    port [..]           Manage or show port status. ...
    ptp                 System PTP commands.
    rmon                Enter RMON mode
    show spanning-tree  Status of Spanning Tree (RSTP). ...
    show vlan [vid]     IEEE 802.1Q VLAN
    date [..]           System date & time ...
    logout              Logout, or quit the CLI.
    system-information  Show system information
    uptime              Display system uptime
    version             Show currently running firmware build details
    watchdog            Show watchdog status, raw
    whoami              Show user ID.
    ______________________________________________________________________________
    See "help all" or "help COMMAND" for more online help.
    hostname:/#>

Similarly this is a list of commands available to a built-in user having an operator role.

    hostname:/#> whoami
    oswald (operator)
    hostname:/#> help
    show aggregates     Status of aggregated ports
    show alarm [log]    Alarm status, or show alarm log
    show arp            Show CPU ARP cache
    clear               Clear screen.
    show dhcp-clients   Show active DHCP clients. ...
    show sensor         Display environment status: temperature, power, digital in and SFP ...
    show fdb            Forwarding database (ATU/MAC)
    show partitions     Show partition table
    show history        Show command history
    ip <igmp|ospf|..>   System IP mode commands
    show iface [..]     Interface overview
    show lldp           LLDP/CDP neighbours
    show monitor [ID]   Port Monitor Overview
    port [..]           Manage or show port status. ...
    ptp                 System PTP commands.
    rmon                Enter RMON mode
    show spanning-tree  Status of Spanning Tree (RSTP). ...
    show vlan [vid]     IEEE 802.1Q VLAN
    ipcalc <..>         An IP subnet calculator ...
    ping <..>           Ping a network host or group. ...
    show logfile        System default log file, log://messages ...
    nslookup <..>       Query the nameserver for the IP address of the given HOST optionally using  ...
    media [..]          Media related operations. ...
    date [..]           System date & time ...
    logout              Logout, or quit the CLI.
    show memory         Display memory usage
    show processes      Display running processes
    system-information  Show system information
    uptime              Display system uptime
    version             Show currently running firmware build details
    watchdog            Show watchdog status, raw
    whoami              Show user ID.
    ______________________________________________________________________________
    See "help all" or "help COMMAND" for more online help.
    hostname:/#>

« Previous Next »